INDEX: COMMERCIAL AND INDUSTRIAL TRIMS & FLASHINGS
This drawing index provides drawing links to AEP Span’s standard Commercial and Industrial trims & flashings.
Note that most trims are provided in a 10’‐3” length.
Please refer to the C & I Building Systems: Installation, Flashings and Details Guide for application information.

RIDGE, PEAK, HIP TRIMS
ID: PF16
INFO: PEAK USE:	ID: R6
INFO: FORMED RIDGE
USE: SSP	ID: R8
INFO: RIDGE USE:	ID:  R11
INFO: FORMED RIDGE
USE: HR	
ID:  R43
INFO: FORMED RIDGE
USE: BR				

GABLE TRIMS
ID: G6
INFO: 4x5 1/4 GABLE
USE:	ID: G7
INFO: SCULP. GABLE
USE:	ID: G8
INFO: 5x5 1/4 GABLE
USE: SSP, PBR	ID: G9
INFO: SCULP. GABLE
USE: HR	
ID: G12	ID: G15	ID: G19	ID: GE1	
INFO: 5 1/2"	INFO: ALT.	INFO: 4 3/4"	INFO: SCULP.	
GABLE	SCULP. GABLE	GABLE	END CAP	
USE:	USE:	USE:	USE:	

END WALL, SIDE WALL TRIMS
ID: EW6	ID: SW6	ID: SW7	ID: SW8	
INFO:	INFO: 	INFO: 5"	INFO: OPT. 5"	
ENDWALL	SIDEWALL	SIDEWALL	SIDEWALL	
USE:	USE:	USE: SSP, PBR	USE:	

EAVE TRIMS
ID: E6	ID: E7			
INFO: 4x4"	INFO: SCULP.			
EAVE	EAVE			
USE:	USE:			

BASE, DRIP TRIMS
ID: B1
INFO:  1" USE: NW, UP	ID: B6
INFO: 1 5/8" USE:			

JAMBS, C‐METALS
ID: C6
INFO: 1 3/8" USE: SSP, PBR	ID: C7
INFO: 2 1/8" USE:	ID: C11
INFO: 1 5/8" USE: BR, HR	ID: C12
INFO: 1 1/2" USE: MVB	
ID: C13	ID: J6	ID: J8	ID: J11	
INFO: 1"	INFO: 1 3/8"	INFO: 2 1/8"	INFO: 1 5/8"	
USE: NW, UP	JAMB	JAMB	JAMB	
	USE: SSP, PBR	USE:	USE: BR, HR	

ID: J12	ID: J13			
INFO: 1 1/2"	INFO: 1"			
JAMB	JAMB			
USE: MVB	USE: NW			

INSIDE & OUTSIDE CORNERS
ID: IC6
INFO: 5x5" INS. CORNER USE:	ID: IC7
INFO: 4x4" INS. CORNER USE: SSP, PBR	ID: IC11
INFO: 7x7" INS. CORNER USE:	ID: OC6
INFO: 5x5" OUT. CORNER USE: SSP	
ID: OC7	ID: OC11	ID: IC2	ID: OC2	
INFO: 4x4"	INFO: 7x7"	INFO: 3 1/2"	INFO: 3 1/2"	
OUT. CORNER	OUT. CORNER	INS. CORNER	OUT. CORNER	
USE:	USE:	USE:	USE:	

GUTTERS
ID: GS6	ID: GU6	ID: GU7	ID: GU8	
INFO: GUTTER	INFO: BOX,	INFO: SCULP.,	INFO: BOX,	
STRAP	PRE‐HUNG	PRE‐HUNG	POST‐HUNG	
USE:	USE:	USE:	USE:	
ID: GU9	ID: GUE1	ID: GUE2	ID: GUJ1	
INFO: SCULP.,	INFO: BOX	INFO: SCULP.	INFO: EXPAN.	
POST‐HUNG	END CAP	END CAP	JOINT SLEEVE	
USE:	USE:	USE:	USE:	
ID: GUJ2	ID: GUS1	ID: GUS2		
INFO: SCULP.	INFO: BOX	INFO: SCULP.		
JOINT SLEEVE	INSIDE SPLICE	INSIDE SPLICE		
USE:	USE:	USE:		

DOWNSPOUTS
ID: D6	ID: D7	ID: DD6	ID: DD7	
INFO: 3"	INFO: 3x3.7"	INFO: 3"	INFO: 3x3.7"	
DOWNSPOUT	DOWNSPOUT	DROPOUT	DROPOUT	
USE:	USE:	USE:	USE: NW, UP	
ID: DE6	ID: DE7	ID: DE8	ID: DE9	
INFO: 45°	INFO: 70°	INFO: 90°	INFO: 3x3.7"	
ELBOW	ELBOW	ELBOW	45° ELBOW	
USE:	USE:	USE:	USE:	
ID: DE10	ID: DE11	ID: DS6	ID: DS7	
INFO: 3x3.7"	INFO: 3x3.7"	INFO: D.SPOUT	INFO: D.SPOUT	
70° ELBOW	90° ELBOW	OUTSIDE STRAP	INSIDE STRAP	
USE:	USE:	USE:	USE:	
ID: DS8	ID: DS9			
INFO: 3x3.7"	INFO: 3x3.7"			
OUT. STRAP	INSIDE STRAP			
USE:	USE:			

MISC
ID: V6
INFO: VALLEY USE:				
BR: Box Rib HR: HR‐36 MVB: Mini‐V‐Beam NW: Nu‐Wave Corrugated SSP: Super‐Span UP: U‐Panel

CItrimIndex.xlsx	
9/11/2018

NAME: BASE	TRIM
IDENTIFICATION: BHP-MFG-4218
PART # : Bl GIRTH : 4" PTD
ZA
MATL. STROKES: 5

REFERENCE: LT. GAUGE

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FOR CODES)

"\
B1
XXX
MODIFIER
COLOR PAINT TYPE GAUGE PART PANEL

 	 IF   PAINTED,
THIS  SIDE

2 1/8"

1 "

135"

3/8" HEM

 	

 	

				

				

				

NAME: DRIP	EDGE

□

IDENTIFICATION: ASC-MFG-5049

"\
REFERENCE:MTL.   BLDGS	B6

PART # : B6 GIRTH : 7" PTD
ZA
MATL. STROKES: 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DRIP1.62X
'--v-"

XXX
'--v-"I L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

 	 IF  PAINTED,
THIS  SIDE

4 1/8'

/-1 5/8'-,"

7

135°

3/4'
'

/2'	HEM

 	

	

				

				

				

"\

C6

NAME: 1	3/8"	C-METAL
IDENTIFICATION:   ASC-MFG-4844	REFERENCE: MTL. BLDGS

PART # : C6 GIRTH : 7" PTD
ZA
MATL. STROKES: 5

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

CMETl.3 2X
'--y-/

XXX
'--y-/l L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

3   7/8°

IF PAINTED,
THIS SIDE

I

t
1   3/8°
i

1   1/4'

 	

	

				

				

				

r	"\

.,J

C7

"\

NAME: 2	1/8"	c- METAL

□

IDENTIFICATION:    ASC-MFG-4843	REFERENCE: INDUSTRIAL

PART # : C7 GIRTH	: 9 PTD
ZA
MATL. STROKES: 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

CMET2.12X
'--y-/

XXX
'--y-/l L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE
,

I

4,5000

2.1250
I	

1.8750

 	

	

				

				

				

NAME: 1	5/8"	C-METAL

□

IDENTIFICATION:    ASC-MFG-4846	REFERENCE: INDUSTRIAL

"\
Cll

PART # : C11 GIRTH	: 7 PTD
ZA
MATL. STROKES: 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

CMETl.6  2X
'--v-"

XXX
'--v-"I L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF  PAINTED,
/THIS SIDE

3 1/2#

i

1

5 / 88

rl	3/8'-/

1

 	

	

				

				

				

NAME: 1	1/2"	C-METAL
IDENTIFICATION:   ASC-MFG-4845	REFERENCE: INDUSTRIAL

C12	'

PART # : C12 GIRTH	: 7" PTD
ZA
MATL. STROKES: 5

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

CMETl.5  2X
'--y-/

XXX
'--y-/l L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE

I
3  3/4#

1  1/ 28

 	

	

				

				

				

r

.,J

NAME: 1"	C-METAL	&
IDENTIFICATION:   ASC-MFG-5029	REFERENCE: INDUSTRIAL

"\
C13

PART # : C13 GIRTH	: 6"	£

□

DESCRIPTION F STANDARD

CMETl	2X
'--y-/

XXX

I 	

'--y-/l L  

MODIFIER

PTD
ZA
MATL. STROKES: 5

i

&

1

,+1/8°
-OH
t	

PART NUMBERS (SEE INDEX FDR CODES)

&
3  1/2°

'

COLOR
PAINT TYPE GAUGE PART PANEL

IF PAINTED,
THIS SIDE

/-lH	7"

				

				

				

				

r	"\

"\

D6

NAME:DOWN	SPOUT	3"
IDENTIFICATION:     IMSA-MFG-4837	REFERE NCE : MTL. BLDGS.

PART # : D6
GIRTH	: 15" BENCH WORK
PTD
ZA
MATL .
S TR OKE S : 8

DESCRIPTION	DS

□

F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

2X
'	/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE

 	

	

				

				

				

r

D7

NAME:DOWN	SPOUT	3"	x	3.7"

□

IDENTIFICATION:   IMSA-MFG-4974	REFERENCE: MTL. BLDGS.

"'\

PART # : D7
GIRTH	: 14.125" BENCH WORK

DESCRIPTION F STANDARD

DS3.7	2X
'--y-/

XXX

I 	

'--y-/l L  

MODIFIER

PTD
ZA
MATL. STROKES: 8

PART NUMBERS (SEE INDEX FDR CODES)

3 ll/16H

IF PAINTED, THIS SIDE

COLOR
PAINT TYPE GAUGE PART PANEL

3  ll/16H

 	

	

				

				

				

NAME: DOWN	SPOUT	DROPOUT

□

IDENTIFICATION:    IMSA-MFG-4539	REFERENCE: MTL. BLDGS.

DD6

"'\

PART # : DD6
GIRTH	: BENCH WORK
PTD
ZA
MATL.
STROKES:BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSDO	2X
'--y-/

XXX
'--y-/l L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

l/2H FLANGE

IF PAINTED,  	  THIS SIDE

\

2

3/4H	7"

\

 	

	

				

				

				

NAME: DOWN	SPOUT	DROPOUT

3x3.7

"'\

□

IDENTIFICATION: IMSA-MFG-4975

REFERENCE: MTL. BLDGS.

DD7

PART # : DD7
GIRTH	: BENCH WORK
PTD
ZA
MATL.
STROKES:BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSD07 2X
'--y-/

XXX
'--y-/l L  

I 	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

1/28        FLANGE

IF PAINTED,  	
THIS SIDE

\

7 / 168

/-2

3 / 48  -------7"

\

 	

	

				

				

				

NAME: DOWN	SPOUT	ELBOW	45°
IDENTIFICATION:     IMSA-MFG-4838	RE FERE NCE : MTL. BLDGS.

"\
DE6

PART # : DE6
GIRTH	: BENCH WORK PTD
ZA
MATL   . STROKES:BENCH WORK

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB45 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"
K
4"

\

□

SEAM THIS SIDE UNLESS	THER I SE SPECIFIED,

				

				

				

				

r	"\

NAME: DOWN	SPOUT	ELBOW	70°
IDENTIFICATION:     IMSA-MFG-4980	RE FERE NCE : MTL. BLDGS.

"\
DE7

PART # : DE7
GIRTH	: BENCH WORK PTD
ZA
MATL   . STROKES:BENCH WORK

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB70 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"
K
4"

\

□

SEAM THIS SIDE UNLESS	THER I SE SPECIFIED,

				

				

				

				

r	"\

"\
NAME: DOWN	SPOUT	ELBOW	90°

IDENTIFICATION: IMSA-MFG-4981

REFERENCE: MTL. BLDGS.

DEB

PART # : DEB
GIRTH	: BENCH WORK PTD
ZA
MATL.
STROKES:BENCH WORK

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB90 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"
'f(

4"

\

□

SEAM THIS SIDE UNLESS	THER I SE SPECIFIED.

				

				

				

				

r	"\

"\
NAME:DOWN	SPOUT	ELBOW	3"	X	3.7"	45°

IDENTIFICATION: ASC-MFG-4976

□

RE FERE NCE : MTL. BLDGS

DE9

PART # : DE9
GIRTH	: BENCH WORK PTD
ZA
MATL .

S TROKES : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB745 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"

11/16"

\

3

□

SEAM THIS SIDE UNLESS	THER I SE SPECIF I ED,

 	

	

				

				

				

NAME:DOWN	SPOUT	ELBOW	3"	X	3.7"	70°

"'\

IDENTIFICATION: ASC-MFG-4982

□

RE FERE NCE : MTL. BLDGS

DElO

PART # : DEl0
GIRTH	: BENCH WORK PTD
ZA
MATL .

S TROKES : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB770 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"

11/1

\

3

□

SEAM THIS SIDE UNLESS	THER I SE SPECIFIED.

 	

	

				

				

				

"\
NAME:DOWN	SPOUT	ELBOW	3"	X	3.7"	90°

IDENTIFICATION: ASC-MFG-4963

□

REFERE NCE : MTL. BLDGS

DEll

PART # : DEll
GIRTH	: BENCH WORK
PTD
ZA
MATL .

S TR OKE S : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSELB790 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,

3"

11/16"

\

3

□

SEAM THIS SIDE UNLESS	THER I SE SPECIFIED,

 	

	

				

				

				

NAME: DOWN	SPOUT	OUTSIDE

STRAP

"\

□

IDENTIFICATION:    IMSA-MFG-4840	REFERE NCE : MTL. BLDGS.

DS6

PART # : DS6 GIRTH	: 13 1/4" PTD
ZA
MATL .
S TR OKE S : 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSSOS 2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

4 1/W

IF PAINTED, THIS SIDE

3  1/16'	1/16'

1 1/

 	

	

				

				

				

NAME: DOWN	SPOUT	INSIDE	STRAP

IDENTIFICATION: IMSA-MFG-4841

"\

□

REFERE NCE : MTL. BLDGS.

DS7

PART # : DS7 GIRTH	: 9 1/8" PTD
ZA
MATL .
S TR OKE S : 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSSIS	2X
'	/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

I

4 1/8°

20
I	

IF PAINTED,
THIS SIDE

1   1/	 	

 	

	

				

				

				

NAME: DOWN	SPOUT	OUTSIDE	STRAP	3x3.7

"\
DSB

□

IDENTIFICATION:     IMSA-MFG-4977	REFERE NCE : MTL. BLDGS.

PART #  : DS8 GIRTH	: 12 15/16" PTD
ZA
MATL .
S TR OKE S : 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSS0S72X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

3 13/16#

IF PAINTED, THIS SIDE

<1  1/

 	

	

				

				

				

NAME: DOWN	SPOUT	INSIDE	STRAP	3x3.7
IDENTIFICATION:     IMSA-MFG-4978	REFERE NCE : MTL. BLDGS.

"\

□

DS9

PART # : DS9 GIRTH	: 8 13/16" PTD
ZA
MATL .
S TR OKE S : 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

DSSIS7 2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

I

3 13/16°

20
I	

IF PAINTED, THIS SIDE

1   1/	 	

 	

	

				

				

				

NAME: 4"	x	4"	EAVE
IDENTIFICATION: ASC-MFG-4852

□

REFERENCE:MTL.

"\
HLDGS	E6

PART # : E6 GIRTH	: 11" PTD
ZA
MATL. STROKES: 5

I

5 3/4°

DESCRIPTION F STANDARD PART NUMBERS CSEE INDEX FDR CODES)

EAV4X4 2X
'--y--/

XXX
'--y--/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

I

IF  PAINTED,
;THIS SIDE

y
<112n HEM

 	

	

 			

 			

 			

			

  			

 			

 			

  			

  			

  			

r

\.

"\

E7

NAME: SCULPTURED	EAVE
IDENTIFICATION:    ASC-MFG-4850	REFERENCE: MTL. BLDGS

PART  #	E7 GIRTH	17" PTD
ZA
MATL. STROKES 7

DESCRIPTION OF STANDARD PART NUMBERS CSEE INDEX FDR CODES)

EAVS	2X
'-v--"

XXX

I  	

'-v--"I L 	MODIFIER COLOR PAINT TYPE GAUGE
PART PANEL

-
IF PAINTED,
THIS SIDE

\

\..
1/2	HEM

SLOPE	0.	b	S,O,	
1:12	129°			
2:12	132°			
3:12	134°			
4:12	138°			
5:12	143°			
6:12	14r			
7:12	150°			
8:12	154°			
9:12	15r			
10:12	160°			
11:12	163°			
12:12	165°			

'\

1

DIE OPENING

RAM SPEED

RAM OPEN

ANGLE

DIMENSIDN

STATION

SPECIAL  INSTRUCTIONS

2

3

4

5

6

7

8

9

10

P  -  PAINTED   /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES. TOLERANCE: ± 1/8"
± 2·

r

SLOPE CONVERSION CHART
J

"\

J

"\
NAME: ENDWALL	TRANSITION

IDENTIFICATION: ASC-MFG-4928

REFERENCE:MTL.

HLDGS

EW6

PART # : EW6

DESCRIPTION

ENDWTRN	2X XXX

GIRTH	: 11"
PTD

□F STANDARD
RS

'---y-/

'---y-/l L  

MODIFIER COLOR

ZA
MATL. STROKES: 4

PART NUMBE
CSEE INDEX FDR CODES)

PAINT TYPE
1 	GAUGE
PART PANEL

4 112°

112° HEM

				

				

				

				

"\

G6

NAME:4"	x	5	1/4"	GABLE	RIM

□

IDENTIFICATION:     IMSA-MFG-4820	REFERE NCE : MTL. BLDGS

PART # : G6 GIRTH	: 13 3/8" PTD
ZA
MATL .
S TR OKE S : 9

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GAB5.2f:eX
'--v-"

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

40

'

IF PAINTED, THIS SIDE

_J
8

7/8°
'	'	8

5 1/4°
8

1 3/4°

r---r--3/8° HEM

3/4'_/	'

3/8° HEM

 	

	

				

				

				

"\

G7

NAME: SCULPTURED	GABLE	TRIM
IDENTIFICATION:    IMSA-MFG-4863	REFERENCE: MTL. BLDGS.

PART # : G7 GIRTH	: 17 7/8" PTD
ZA
MATL . STROKES: 11

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GABS	2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

1/2°

IF PAIN TED,
-THIS SIDE
\

1/2°

				

				

				

				

r	"\

r	Re
NAME: 5"	X	5	1/4"	GABLE	TRIM
IDE NTIF ICATION :	ASC-MFG-4966	RE FERE NCE : MTL. BLDGS.	turn to Menu	"\
G8	
	
PART	# : GB
GIRTH	: 14 1/2"
PTD ZA MATL .
S TROKE S: 9	DES OF PAR (SE FOR	CRIPTION STANDARD
T NUMBERS E INDEX
CODES)	XXX
MODIFIER COLOR PAINT TYPE GAUGE PART  PANEL	

5	

IF PAINTED, THIS SIDE

1/4"

3/4"	I	

'	

(	

1 /2"	

4 7/8"

HEM	

1/2" HEM		
	
STATION	DIMENSION	ANGLE	RAM OPEN	RAM SPEED	DIE OPENING	SPECIAL INSTRUCTIONS	SLOPE	a	b	S.O.	
1											
											
2											
												
3												
												
4												
												
5												
												
6												
												
7												
												
8												
												
9												
												
10											

P  -  PAINTED   /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES . TOLERANCE : ± 1/8"
± 2°					
	SLOPE CONVERSION	CHART	
,,I	

r

"\

□

IDENTIFICATION: ASC-MFG-4969

REFERENCE: MTL. BLDGS.

NAME: SCULPTURED	GABLE	TRIM	5"	G9

PART # : G9 GIRTH	: 21 1/2" PTD
ZA
MATL . STROKES: 11

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GABS	2X
'--v-"

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

H

1/2°

-

 	'

 		 	 IF  PAINTED,
THIS SIDE
\

1/2°

5/8°"'HEM

				

				

				

				

r

NAME: 5	1/2"	GABLE	TRIM

"\
G12

IDENTIFICATION:   ASC-MFG-4965	REFERENCE: INDUSTRIAL

PART # : G12 GIRTH : 11" PTD
ZA
MATL . STROKES: 7

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GAB5.5 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

t	

'

IF PAINTED, THIS SIDE

_J

3   3 / 48

 	t

,
Wl/28        HEM

5   1/  28
8
3/4'_/

1/2u  HEM

 	

	

				

				

				

r	"\

NAME: SCULPTURED	GABLE	TRIM	E

IDENTIFICATION: ASC MFG-4972

"\

REFERENCE: INDUSTRIAL

GlS

PART # : G15 GIRTH	: 14 1/2" PTD
ZA

MATL. STROKES: 10

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GABE	2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

HH

/2°

1/

\

/2°

IF PAINTED, THIS SIDE

 	

	

				

				

				

r	"\

NAME:4	3/4"	GABLE	TRIM

"\
G19

IDENTIFICATION:   ASC-MFG-4984	REFERENCE: INDUSTRIAL

PART # : G19 GIRTH : 10" PTD
ZA
MATL . STROKES: 7

DESCRIPTION OF STANDARD PART NUMBERS (SEE   INDEX FDR CODES)

GAB4.75 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

3  1/  2 6     	

l-112u HEM

1/2' HE

 	

	

				

				

				

r	"\

NAME: SCULPTURED	GABLE	END	CAP

□

IDENTIFICATION:     IMSA-MFG-5025	RE FERE NCE : MTL. BLDGS.

"\
GEl

PART # : GE1
GIRTH	: BENCH WORK PTD
ZA
MATL .
S TROKES : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GABSEC2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

/ 16 8

8	-

8
IF  PAINTED,   	             THIS SIDE
8

LEFT SIDE SHOWN
SPECIFY RIGHT OR LEFT SIDE

\

/ 168

 	

	

				

				

				

NAME: GUTTER	STRAP
IDENTIFICATION:    IMSA-MFG-5091	REFERE NCE : MTL. BLDGS.

"\

□

GS6

PART # : GS6 GIRTH	: 8 1/2" PTD
ZA
MATL .
S TR OKE S : 2

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTS	2X
'	/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE

I

 	

	

				

				

				

NAME:BOX	GUTTER	(PRE	HUNG)

"\

GLJ6

□

IDENTIFICATION:   ASC-MFG-4834	REFERENCE: MTL. BLDGS

PART # : GU6 GIRTH	: 21 1/2" PTD
ZA
MATL . STROKES: 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTBXPR2X
'---y-/

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

5 5/16°

\

H

				

				

				

				

r

.I

NAME: SCULPTURED	GUTTER	(PRE	HUNG)

□

IDENTIFICATION:    ASC-MFG-4828	REFERE NCE : MTL. BLDGS

GLJ7

"'\

PART# : GU7 GIRTH	: 21 1/2" PTD
ZA
MATL .
S TR OKE S : 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTSPR  2X
'---y-/

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

4 1/4°

/2°

 	

-
IF PAINTED,

THIS SIDE
\

1/2°

				

				

				

				

r

NAME:BOX	GUTTER	(POST	HUNG)

□

IDENTIFICATION:   IMSA-MFG-4963	REFERENCE: MTL. BLDGS

"\

GLJ8

PART # : GUS GIRTH	: 17 3/8" PTD
ZA
MATL. STROKES: 7

DESCRIPTION F STANDARD PART NUMBERS CSEE INDEX FDR CODES)

GUTBXP02X
'	v--"

XXX
'	v--"I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

u

4 3/4°

\

				

				

				

				

r

.I

NAME: SCULPTURED	GUTTER	(POST	HUNG)

□

IDENTIFICATION:   IMSA-MFG-4930	REFERENCE: MTL. BLDGS

"\
GLJ9

PART # : GU9 GIRTH	: 19" PTD
ZA
MATL .
S TR OKE S : 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTSPO	2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

1/  21

-
 	  IF PAINTED,
THIS SIDE
4   3 / 48	\

				

				

				

				

NAME: BOX	GUTTER	END	CAP

□

IDENTIFICATION:     IMSA-MFG-5020	RE FERE NCE : MTL. BLDGS.

"\
GU El

PART # : GUEl
GIRTH	: BENCH WORK PTD
ZA
MATL .
S TROKES : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTBXEC 2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

RIGHT SIDE SHOWN
SPECIFY LEFT OR RIGHT SIDE

4  11/ 168

5 7

'

IF PAINTED,

 	

	

				

				

				

NAME: SCULPTURED	GUTTER	END	CAP

"\
GLJE2

□

IDENTIFICATION:     IMSA-MFG-5019	RE FERE NCE : MTL. BLDGS.

PART # : GUE2
GIRTH	: BENCH WORK PTD
ZA
MATL .
S TROKES : BENCH WORK

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTSEC2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

3 7

\
IF   PAINTED,   	             THIS SIDE

-
3 7/

RIGHT  SIDE  SHOWN	-

4  11/16°

 	

	

				

				

				

NAME:BOX	GUTTER	EXP.	JOINT	SLEEVE

"\
GLJJl

□

IDENTIFICATION:     IMSA-MFG-5026	REFERE NCE : MTL. BLDGS.

PART # : GUJ1 GIRTH	: 15 11/16" PTD
ZA
MATL .
S TR OKE S : 4

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTBXEJ	2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

1

1   1/  48

\

4   13 / 168

5   9 / 168

PAINTED,
IS SIDE

\

4  1/ 168

LENGTH

 	

	

				

				

				

NAME: SCULPT.	GUTTER
IDENTIFICATION: IMSA-MFG-5014

"\

EXP.	JOINT	SLEEVE
REFERE NCE : MTL.   BLDGS.	G lJ J 2

PART # : GUJ2 GIRTH	: 13 7/16" PTD
ZA
MATL . STROKES: 5

DESCRIPTION OF STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTSEJ2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

1 1/ 4H

9 / 16 8
\

)
9 / 168

THIS SIDE

				

				

				

				

r	"\

\.

NAME: BOX	GUTTER	INSIDE	SPLICE

"\
GLJSl

□

IDENTIFICATION:    IMSA-MFG-5021	REFERE NCE : MTL. BLDGS

PART # : GUS1 GIRTH	: 14 7/8" PTD
ZA
MATL .
S TR OKE S : 7

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

GUTBXISP2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

LENGTH	1
\

4 l/2H

/16H

				

				

				

				

r

.I

"\

s

NAME: SCULPTURED	GUTTER	INSIDE	SPLICE
IDENTIFICATION:    IMSA-MFG-5016	REFERENCE: MTL.  BLDGS	G LJ	2

PART # : GUS2 GIRTH	: 15 1/2" PTD
ZA
MATL . STROKES: 4

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

□

I

GUTSISP 2X
'--y-/

XXX

I  	

'--.../I L 		MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

\

7 /16°
\

I

4  11/ 168

THIS SIDE

				

				

				

				

r	"\

\.

NAME: 5"	x	5"	INSIDE	CORNER

□

IDENTIFICATION:     IMSA-MFG-4868	REFERE NCE : MTL. BLDGS.

"\
IC6

PART # : IC6
GIRTH	: 15 3/4"

DESCRIPTION	ICS5 F STANDARD

2X
'	/

XXX
'	/I L  

MODIFIER

PTD
ZA
MATL .
S TR OKE S : 10

PART NUMBERS (SEE INDEX FDR CODES)

COLOR

I  	

PAINT TYPE GAUGE PART PANEL

1 1 3 / 8° HEM

J
3/8° HEM

/
1  3 / 46
/

 	

	

				

				

				

NAME: 4"	X	4"	INSIDE	CORNER

IDENTIFICATION: ASC-MFG-4970

"\

□

REFERE NCE : MTL. BLDGS.

IC7

PART # : IC7 GIRTH	: 14 1/2" PTD
ZA
MATL .
S TR OKE S : 10

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

ISC4	2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

HEM

 	

	

				

				

				

NAME: 7"	X	7"	INSIDE	CORNER

IDENTIFICATION: ASC-MFG-4870

"\

REFERENCE: INDUSTRIAL

ICll

PART # : IC11 GIRTH	: 14 1/2" PTD
ZA
MATL. STROKES: 6

DESCRIPTION	ISC7
□F STANDARD PART NUMBERS
CSEE INDEX FDR CODES)

2X
'--y--/

XXX
'--y--/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

HEM

_J

!
'	l,

IF PAINTED, THIS SIDE

1/2° HEMJ

 	

	

				

				

				

r

\.

"\

J6

NAME: 1	3/8"	JAME	TRIM

□

IDENTIFICATION:     ASC-MFG-4847	REFERE NCE : MTL. BLDGS

PART # : J6 GIRTH : 7" PTD
ZA
MATL .
S TR OKE S : 4

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

JAMTl.3  2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

3   7/8°

IF PAINTED,
/THIS SIDE

-

-	1  1/  46

 	

	

				

				

				

"\

JB

NAME: 2	1/8"	JAMB	TRIM

□

IDENTIFICATION:   ASC-MFG-5105	REFERENCE: INDUSTRIAL

PART # : JB GIRTH	: 9 PTD
ZA
MATL. STROKES: 4

DESCRIPTION F STANDARD PART NUMBERS CSEE INDEX FDR CODES)

JAMT2.12X
'---y-/

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,
THIS SIDE
,

4,5000

I

2.1250
I	

1.8750

 	

	

				

				

				

NAME: 1	5/8"	JAME	TRIM
IDENTIFICATION:   ASC-MFG-4872	REFERENCE: INDUSTRIAL

"\

□

Jll

PART # : J11 GIRTH	: 7 PTD
ZA
MATL. STROKES: 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

JAMTl.6  2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE
PART PANEL

IF   PAINTED,
/THIS SIDE

3  1/2°

1 5/8°

/--	1 3/ 8°-----/

 	

	

				

				

				

NAME: 1	1/2"	JAMB	TRIM
IDENTIFICATION:     ASC-MFG-4800	REFERE NCE : INDUSTRIAL

"\

□

J12

PART # : J12 GIRTH : 7" PTD
ZA
MATL .
S TR OKE S : 5

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

JAMT1.5  2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED,
/THIS SIDE

3   3 / 48

1  1/ 28

 	

	

				

				

				

NAME: 1"	JAME	TRIM	&
IDENTIFICATION:   ASC-MFG-4905	REFERENCE: INDUSTRIAL

"\
J13

PART # : J13 GIRTH	: 6"

&

□

DESCRIPTION F STANDARD

JAMTl	2X
'---y-/

XXX
'---y-/l L  

MODIFIER

PTD
ZA
MATL . STROKES: 5

PART NUMBERS (SEE INDEX FDR CODES)

COLOR

I  	

PAINT TYPE GAUGE PART PANEL

&

 		t	3 1/2°

IF PAINTED,
THIS SIDE

 '	t

_,L------- 1H 	/

				

				

				

				

r

\.

NAME: 5"	x	5"	OUTSIDE	CORNER
IDENTIFICATION:   IMSA-MFG-4228	REFERENCE: MTL. BLDGS.

"\

□

□

C6

PART # : OC6 GIRTH : 16" PTD
ZA
MATL. STROKES: 10

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

OSC5	2X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

5/8'-

3/8' HEM-

J
3/8' HEM

IF   PAINTED,
/THIS SIDE

5/8'
t

				

				

				

				

NAME: 4"	x	4"	OUTSIDE	CORNER

IDENTIFICATION: ASC-MFG-4971

"\

□

REFERE NCE : MTL. BLDGS

□

C7

PART # : 0C7
GIRTH	: 14 1/2"

DESCRIPTION F STANDARD

0SC4X4  2X
'--y-/

XXX
'--y-/l L  

MODIFIER

PTD
ZA
MATL .

5/8°-

S TR OKE S : 10

PART NUMBERS (SEE INDEX FDR CODES)

43/16 	I

COLOR

I  	

PAINT TYPE GAUGE PART PANEL

IF	PAINTED, THIS SIDE

4  3/ 166
1/ 26        HEM-

1/ 26        HEM
t

 	

	

				

				

				

□

C l l

□

"\

NAME: 7"	X	7"	OUTSIDE	CORNER

IDENTIFICATION: ASC-MFG-4950

REFERE NCE : INDUSTRIAL

PART # : OCll
GIRTH	: 14 1/2"

DESCRIPTION F STANDARD

OSC7	2X
'--y-/

XXX
'--y-/l L  

MODIFIER

PTD
ZA
MATL .
S TR OKE S : 6

PART NUMBERS (SEE INDEX FDR CODES)

6 3/4°

IF PAINTED,
THIS SIDE

COLOR

I  	

PAINT TYPE GAUGE PART PANEL

L
1/2°

6 3/4°

l,
1/2° HEMj

				

				

				

				

r	Re
NAME: SKYLINE	PEAK
IDENTIFICATION:  IMSA-MFG-4271	REFERENCE: SKYLINE	turn to Menu	"'
PF16	
	
PART	# : PF16
GIRTH	: (SEE CHART)
PTD ZA MATL.
STROKES: 7	□DESCRIPTION	SKPEAK2X 	XXX
F STANDARD	'---y--/	'---y--/l L 	MODIFIER
PART NUMBERS	I 	COLOR
PAINT TYPE
(SEE INDEX	GAUGE
FDR CODES)	PART
PANEL	

IF PAINTED,
THIS SIDE

'

G	0        HEM
135"

1/2°_/	'

r3/8° HEM	
	
	SLOPE	0.	b	C	S.O.	
	3:12	76"	4 3/8"	5 3/ 4"	11 3/8°	
	4:12	72"	4 3/8"	5 3/ 4"	11 3/8°	
	5:12	6 7"	4 3/8"	5 3/ 4"	11 3/8°	
	6:12	63"	4 3/4"	5 7/8"	11 7/8°	
	7:12	60"	4 3/4"	5 7/8"	11 7/8°	
	8:12	56"	5 1/8°	6 1/8"	12 1/2°	
	9:12	53"	5 l/8°	6 1/8"	12 1/2°	
	10:12	50"	5 5/8"	6 3/8"	13 l/ 4°	
	11:12	4 7"	5 5/8"	6 3/8"	13 l/ 4°	

P  -   PAINTED   /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES. TOLERANCE: ± 1/ 8 "
\.	± 2°	12:12	45"	5 5/8"	6 3/8"	13 1/4"	
	SLOPE CONVERSION CHART
,,J	

\

r	"'\

,,J

NAME: SUPER-SPAN	FORMED

"\
RIDGE	R6

□

IDENTIFICATION:     IMSA-MFG-4821	REFERE NCE : MTL. BLDGS.

PART # : R6 GIRTH : NA PTD
ZA
MATL . STROKES: NA

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

RIDFSSP 1X
'-----/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE
'

NAME: RIDGE/HIP
IDENTIFICATION: ASC-MFG-5034

"\
REFERENCE: MTL.  BLDGS	RB

PART # : RB GIRTH	: 21 1/2" PTD
ZA
MATL. STROKES: 6

DESCRIPTION F STANDARD

□

PART NUMBERS (SEE  INDEX FDR CODES)

RIDHIP 2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

IF PAINTED, THIS SIDE

AT RIDGE

....--3/4° HEM

AT HIP

3/4° HEM-...

				

				

				

				

□

REFERE NCE : INDUSTRIAL

NAME: HR-36	FORMED	RIDGE

IDENTIFICATION: ASC-MFG-4822

Rll

"'\

PART # : Rll
GIRTH	: 30" OR 36"
PTD
ZA
MATL .
S TR OKE S : DEP ENDS ON PITCH
IF PAINTED, THIS SIDE

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

RIDFHR36
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

'

158 DR 1B8 ---

				

				

				

				

NAME: SIDEWALL
IDENTIFICATION:     IMSA-MFG-4929	REFERE NCE : MTL. BLDGS.

"\

□

SW6

PART # : SW6 GIRTH	: 11 3/8" PTD
ZA
MATL .
S TR OKE S : 6

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

SIDW	2X
'	/

XXX
'	/I L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

4 1/8°

2 1/8°

IF PAINTED, THIS SIDE

'
w3/8° HEM

				

				

				

				

NAME: SIDEWALL	5"
IDENTIFICATION: ASC-MFG-4973

REFERE NCE : MTL. BLDGS

"\

□

SW7

PART # : SW7 GIRTH	: 14 1/2" PTD
ZA
MATL .
S TR OKE S : 6

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

SIDW	2X
'---y-/

XXX
'---y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

5 5 / 8°

JNTED,
SIDE

2  1/8°

				

				

				

				

r	"\

NAME: SIDEWALL	(OPTIONAL)	5"

□

IDENTIFICATION:   IMSA-MFG-4979	REFERENCE: MTL. BLDGS.

SWB

"'\

PART # : SW8 GIRTH	: 10 3/4" PTD
ZA
MATL. STROKES: 4

DESCRIPTION F STANDARD PART NUMBERS (SEE INDEX FDR CODES)

SIDWO	2X
'--y-/

XXX
'--y-/l L  

I  	

MODIFIER COLOR PAINT TYPE GAUGE PART PANEL

 	

_)

5 1/4#

-j	f-1;2n HEM

NOTE: FDR 14' - 3n LENGTHS MAKE T\./0 S\./8 SIDE\./ALL FLASHINGS OUT

 	

	

				

				

				

r

 	  	

    	

 	
GIRTH	:  42   15/16"	□F	STANDAR
PTD	PART  NUMBE
ZA	CSEE INDEX
MATL.
STROKES: 4	FDR CODES

 

20   3 / 46

I

SPECIFY ANGLE \./HEN	
STATION	DIMENSIDN	ANGLE	RAM OPEN	RAM SPEED	DIE OPENING	SPECIAL INSTRUCTIONS	
1							
2							
3								
4								
5								
6								
7								
8								
9								
10							

P -  PAINTED  /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES. TOLERANCE: ± 1/8"
±  2"	

D	'	v--"I L  
RS

MODIFIER COLOR

)

IF PAINTED, THIS SIDE

 	  PAINT TYPE
GAUGE PART PANEL

20   3 / 46

ORDERING

 	SLOPE	0.	b	S,O,	
1: 12	131'			
2:12	128'			
3:12	125			
4:12	122·			
5:12	119'			
6:12	117'			
7:12	114'			
8:12	112·			
9:12	11o·			
10: 12	108'			
11:12	107'			
12:12	105'			
SLOPE CONVERSION CHART
J
r	"\

J

r	Re
NAME: BOX	RIB	FORMED	RIDGE
IDE NTIF ICATION :	ASC-MFG-7028	RE FERE NCE : INDUSTRIAL	turn to Menu	"\
R43	
	
PART	# : R43
GIRTH	30" OR 36"
PTD
ZA
MATL .
S TROKE S: DEP ENDS ON PITCH	□DESCRIPTION	RIDFBRR 	XXX
F STANDARD	'--y--/	'--y--/l L 	MODIFIER
COLOR
PART NUMBERS	I 	PAINT TYPE
(SEE INDEX	GAUGE
PART
FDR CODES)	PANEL	

IF PAINTED, THIS SIDE	
	
STATION	DIMENSION	ANGLE	RAM OPEN	RAM SPEED	DIE OPENING	SPECIAL INSTRUCTIONS	SLOPE	Cl	b	S.O.	
1											
							3:12	152°			
2											
								4:12	143°			
3												
								5:12	135°			
4												
								ANY PITCH BEYOND  5:12  WILL  RESULT IN MATERIAL BEING DAMAGED	
5									
6									
												
7												
												
8												
												
9												
												
10											

P   -  PAINTED   /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES . TOLERANCE: ± 1/8"
±  2·					
	SLOPE CONVERSION CHART
J	

r

\.

r	Re
NAME: UNIVERSAL	OUTSIDE	CORNER
IDENTIFICATION:    BHP-MFG-4235	REFERENCE: LT. GAUGE	turn to Menu	"'
OC2	
	
PART	# : OC2
GIRTH	: 7 3/ 4"
PTD ZA MATL.
STROKES: 6	DESCRIPTION	XXX
OF STANDARD	MODIFIER
PART NUMBERS	COLOR
PAINT 1YPE
(SEE INDEX	GAUGE
PART
FOR CODES)	PANEL	

3  1/2"
IF PAINTED, THIS SIDE

L

3/8" HEM+--/

3 1/2"

}	L
3/8" HEM	
	
STATION	DIMENSION	ANGLE	RAM OPEN	RAM SPEED	DIE OPENING	SPECIAL INSTRUCTIONS	SLOPE	a	b	S.O.	
1											
											
2												
												
3												
												
4												
												
5												
												
6												
												
7												
												
8												
												
9												
												
10												

P  -  PAINTED  /  EXPOSED   SIDE ALL DIMENSIONS ARE IN IN CHES . TOLERANCE: ± 1/8"
\.	± 2·					
	SLOPE CONVERSION	CHART
,,I	

\

r	"'\

r	Re
NAME: UNIVERSAL	INSIDE	CORNER
IDE  NT IF ICATION:    BHP-MFG-4433	REFERE NCE : LT. GAUGE	turn to Menu	"\
IC2	
	
PART	# : IC2
GIRTH	: 7 3/4"
PTD ZA MATL .
S TROKE S : 6	DESCRIPTION	XXX
OF STANDARD	MODIFIER
PART NUMBERS	COLOR
PAINT TYPE
(SEE INDEX	GAUGE
PART
FOR CODES)	PANEL	

3  1/2"

r----r 3/8" HEM
--,
_J

3 1/2"

IF PAINTED, THIS SIDE
L	
	
STATION	DIMENSION	ANGLE	RAM OPEN	RAM SPEED	DIE OPENING	SPECIAL INSTRUCTIONS	SLOPE	a	b	s.o.	
1											
											
2												
												
3												
												
4												
												
5												
												
6												
												
7												
												
8												
												
9												
												
10												

P  -   PAINTED   /   EXPOSED   SIDE ALL DIMENSIONS ARE IN INCHES. TOLERANCE: ± 1/ 8 "
±  2·					
	SLOPE  CONVERSION	CHART
,,I	

r