-    PANEL  CLIP		
APPLY CURING SEALANT					
TO BOTH SIDES OF RIB PRIOR TO INSTALLING			- DESIGN SPAN HP PANEL		

RIB COVER -					

DESIGN CAUTION:					
ROOF SLOPE TRANSITIONS S					
AS FASCIAS MAY ESTABLISH					
UNWANTED POINT OF PANEL
FIXITY. CONTACT YOUR AEP SPAN REPRESENTATIVE FOR ASSISTANCE.	I  I
I  I
I  I
I  I				
	I I				
	I l""""o		PANEL RIBS		
1/8" RIVET - BOTH SIDES	I I I I
I		D OVER EDGE. SEAL
DS OF ROOF PANEL RIBS RING SEALANT
INSTALLING RIB COVER		
	I				
	:J				
DESIGN SPAN HP PANEL -			UNDERLAYMENT		
			(NOT BY AEP-SPAN)		

PANEL CLIP			
-   SUBSTRATE		
(CONTACT AEP-SPAN FOR -					
CLIP LOCATION & SPACING)					
			-    PANCAKE HEAD		
			FASTENERS		
1/4" MIN. CLEARANCE FOR WEEPAGE	
 			
FIELD NOTCH AND HEM 1"		
			(OPTIONAL FACTORY		
			PANEL  NOTCH)		
DRIP FLASHING (DF009)		
--	SHOULD BE MINIMUM ¼" GREATER		
			THAN  PANEL  RIB  HEIGHT.		
NOTE:					
THE USE OF THIS DETAIL IS NOT					
RECOMMENDED IN SNOW CLIMATES.					
  	 	r	 	
    	-	 N
A Bluescope Steel Company
\._		DESIGN SPAN	HP
-II-	 	1 	
FASCIA TRANSITION/ WALL	
			ind	DS-07	

_)	

REV. 11/15/12