Title: C:\Users\goughbrian\Desktop\Installation Details - Master Files\Design Span hp\2012 Rework Pending\Design Span hp - ALL DETAILS
Author: goughbrian

RIDGE CAP

1/8"	RIVETS IN SEALANT LINE
IF NECESSARY TO CLOSE "FISHMOUTH"

f
)I
,,11,11,11,,,I ---

WIDE
_t	BATTEN CAP

(_	SPECIFIED UNDERLAYMENT (NOT BY AEP-SPAN)

EQUALLY SPACED FASTENERS*
(3) MIN. FOR 12 "
(4) MIN. FOR 16", 17" & 18"

NOTE:
* ADDITIONAL FASTENERS MAY BE REQUIRED IN HIGH SNOW LOAD AREAS. SEE APPENDIX.

1/8" RIVETS | | |
@ 12" o.c. | | |
| ·' | |
| I | |
3/16"x7/8" | | |
CONTINUOUS | | |
BUTYL TAPE | | |
(ZC219) | | |
NOTCH AROUND PANEL RIBS. | | |
USE NON-SKINNING BUTYL | | |
SEALANT AROUND NOTCH | | |
FOR   PANEL  RIB. | | |
WIDE BATTEN STOPS | | |
AT   ZEE CLOSURE | | |
DESIGN SPAN HP PANEL | | |

A Bluescope Steel Company
\._

DESIGN SPAN	HP

RIDGE/ HIP (WIDE BATTEN)

ind | DS-14 | _)

REV. 11/15/12