r			

I I .•.•
I . .
I .
------- --+·7 -
·.·. 1
,·	I
.Jr.	I	I
'T'	1 :-	:
I • .
I	I
1- ::- :
I			

SPECIFIED					
	UNDERLA YMENT (X)					
	SUBSTRATE					
	TRIM FASTENER W/SEALING					
	WASHER OR RIVET					
	CONTINUOUS BEAD OF NON­					
	SKINNING BUTYL TAPE OR SEALANT					
	UNDER COVER PERIMETER					
	SEAL PENETRATION PERIMETER					
	WITH POLYURETHANE SEALANT					
	WALL  PENETRATION

OVERLAPPED PENETRATION COVER			-,--		
				1		
				I		
	PROVIDE SUFFICIENT CLEARANCE BETWEEN FLASHING & PENETRATION  TO ACCOMODATE THERMAL MOVEMENT.			I I
I I		
				I		
				I		
				I		

(X) - NOT BY AEP SPAN					

I...	  	 	r	 	
N	FLUSH PANEL
HORIZONTAL INSTALL.
J	J_	
WALL PENETRATION	
					FPH-17	

.)	

REV. 9/23/16