r

1 1/2"

135 ·
5/ 8"

TC209

1/ 4: 12 MIN. SLOPE

PARAPET FLASHING (V) BLOCKING (AS REQUIRED)

TRIM CLEAT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

SPECIFIED UNDERLA YMENT (X)

SUBSTRATE

1 ••

I . •.•
I . .
I • • 1-  .. .
I. .

..

-1         .
I    •   •

I .  .
I    •  •
1 • .•.
I. .
1 •  •
I • •

I- .. I.   .

-1           .
I . •.•
I . .

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS

FLUSH PANEL
VERTICAL INSTALL.
J	J_

PARAPET

FPV-12

I...

.)
REV. 11/16/18