Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Flush Panel\Sep16 Pending Ne
Author: goughbrian

r | | | | |
| | | | 1/2" |
| | | | 135· |
| | | | 4" |
| | | | 1/2" |
| | | | 1 1/2" |
| | | L	J	l ~~J~~ | |
| | | ----f---7 | |
| | | • I | |
| | | . · 1 | | WALL CLOSURE (WC217)
| | | . · 1 | |
| | | • I .  ^. ^.·1 | | TRIM FASTENER W/SEALING WASHER OR RIVET AT 12 " O.C. MAXIMUM
| | | • I | |
| | | . · 1 | | CONTINUOUS BEAD OF NON­
| | | | | SKINNING BUTYL TAPE OR SEALANT
| | | . ·1 | |
| | | • I | | PANEL FASTENER
| | | | | SUBSTRATE
| | | | | SPECIFIED UNDERLA YMENT (X)
| | | . ·1 | |
| | | • I | |
| | | .  ^. ·^.1 | |
| (X) | - | NOT BY AEP SPAN | |
I... | | | r N | J | FLUSH PANEL VERTICAL INSTALL. J_ | | DOOR / WINDOW (SILL)

FPV-15
..)

REV. 9/23/16