Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Wall Panels\Flex Series\2016
Author: goughbrian

r

TOP SIDE CLOSURE FOR ALL PANELS &
CL1.2FX-1P	BOTTOM SIDE CLOSURE FOR 1 . 2FX 10-12
& 1.2FX3O- 12

_CL1.2FX-2P	M  SIDE  CLOSURE  FOR
FX2O-12  &  1.2FX40-12

FOR PANEL HEM

TEAROFF PERFORATED PLUG SECTIONS TO FILL PANEL REVEALS AS REQUIRED

TOP SIDE CLOSURE FOR ALL PANELS.
CL1.5FX-1P	BOTTOM SIDE CLOSURE FOR 1.5FX1O-12
& 1.5FX3O-1 2

_CL1.5F _X- _2 _P	M  SIDE  CLOSURE FOR
5FX20-12   &   1.5FX4O-   12

NOTE:	APPLICATIONS UTILIZING STANDOFF CLIP ALSO REQUIRE UNIVERSAL CLOSURE STRIP (AEP #CLEM1x19 . 68 OR EQUIV.) TO SEAL OFF ADDITIONAL 1/2" PANEL-TO-SUBSTRATE GAP.

N
I...

FLEX SERIES
HORIZONTAL INSTALL.

PANEL CLOSURES

FXH-03
.)

REV. 7/13/16