Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Flex Series\Flex Series - Ho
Author: goughbrian

r

TRIM	DIM  A	USAGE
ZC226	^1  ^1/4"	^1. ^2FX ^FLUSH ^MOUNT ZC22O	1 3/4"	^1.2FX ^W/O.5" ^STANDOFF
^1  ^1/2"	ZC224	1 1/2"	^1.5FX ^FLUSH ^MOUNT
^A	ZC227	^2"	^1. ^5FX ^W/ ^O. ^5" ^STANDOFF

1 1/2"

TRIM	DIM  A	USAGE
_4"	DFO22	1  5/8"	1. 2FX FLUSH MOUNT
DFO23	2 1/8"	1. 2FX W/ O. 5" STANDOFF
DFO24	1   7/8"	1. 5FX FLUSH MOUNT DFO25	2 3/ 8"    1. 5FX  W/ O. 5"  STANDOFF
1''	_A
1/2"
135·

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)

BUTYL FLASHING TAPE (MAS.O25BF)

1 / 8 " THK HORSESHOE SHIM (SHIM.125) OR EQUIVALENT - SEE NOTE 1

Z-METAL

TRIM FASTENER OR RIVET AT 12" O. C. MAXIMUM

DRIP FLASHING

 		p

1. SHIM USED FOR MOISTURE CONTROL
(DRAINAGE)   IN  FLUSH  MOUNT  APPLICATIONS.	^FLEX ^SERIES ^PANELS ^ARE ^INSTALLED
_(X)    _-    _NOT   _BY _AEP  _SPAN	FROM GROUND TO EAVE.

N
I...

FLEX SERIES
HORIZONTAL INSTALL.

BASE

FXH-05
..)

REV. 6/19/17