r
OPTIONAL: 1"W x 1/8"THK FOAM TAPE (MAS .125PE) TO SECURE CLOSURE PLUGS

TOP SIDE CLOSURE INSTALLATION

TOP CLOSURE
PLUG
SEALANT BE

BOTTOM SIDE CLOSURE INSTALLATION
(FLUSH MOUNTED PANELS)

BOTTOM SIDE CLOSURE INSTALLATION
(PANELS WITH STANDOFF CU

BOTTOM CLOSURE PLUG

1X1 UNIVERSAL CLOSURE STRIP (AEP  #CLEM1X19.68
OR EQUIV.)

NOTES:
- ALL CLOSURE PLUGS SECURED AND SEALED WITH POLYURETHANE SEALANT
(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
VERTICAL INSTALL.	
CLOSURE INSTALLATION	
		FXV-04
..)	

REV. 6/16/17