Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Flex Series\Flex Series - Ve
Author: goughbrian

r

TRIM	DIM  A	USAGE
DFO28	^1  ^1/2"	1. 2FX FLUSH MOUNT DFO29	^2"	1. 2FX  W/ O. 5" STANDOFF
_4"	DFO30	1   3/4"	^1.SFX ^FLUSH ^MOUNT DFO31	2 1/4"	1.SFX  W/ O. 5"  STANDOFF

135· A

1/2"   OPEN HEM

I
I .
I

SUBSTRATE	^I ^•
I ••
SPECIFIED  UNDERLA YMENT (X)	_I
..,..^I_ ^..
BUTYL  FLASHING  TAPE
(MAS.O25BF) PANEL CLIP CLIP FASTENER
INSIDE  CLOSURE  (SEALED  &
SECURED  WITH SEALANT)

DRIP FLASHING

1/4

(X)	-	NOT BY AEP SPAN
(V) - DIMENSION VARIES BASED ON PROJECT CONDITIONS

_(V)	1/2"
1/2"
135"

COVER  TRIM

- _. _. ^. ·_. ^.- _. ^. ·_. ^. ·_. ^. _.· ^. ·_. ^. ·_. ^. ·_. ^. ·_. ^. ·_.
-	 	

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

COVER TRIM

N
I...

FLEX SERIES
VERTICAL INSTALL.

SOFFIT (FRONT)

FXV-10 | .)
REV. 6/16/17