Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Wall Panels\Flex Series\Flex
Author: goughbrian

r

TRIM	DIM A
^1/2"	ZC226	1  1/4"
_135·	_1  _1/2"	ZC22O	^1  ^3/4"
ZC224	1  1/2"
^A	ZC227	^2"

_4"	1 1/2"
^1/2"	--------
1 1/2" WC217

ALTERNATE DETAIL

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
CLIP FASTENER PANEL CLIP

__J	.   .   ._--. 	

ZEE FLASHING CONTINUOUS   BEAD   OF NON­
SKINNING  BUTYL  TAPE  OR  SEALANT

TRIM FASTENER W/SEALING WASHER OR  RIVET  AT  12"   O.C. MAXIMUM

WALL  CLOSURE  (WC217)
NOT BY AEP SPAN

| | | | USAGE |
| | | | 1.2FX FLUSH MOUNT |
| | | | 1.2FX W/O.5" STANDOFF |
| | | | 1.5FX FLUSH MOUNT |
| | | | 1.5FX W/O.5" STANDOFF |
| | | | SEALANT |
| | | | TRIM ANGLE |
| | | | WALL CLOSURE |
| | | | I |
| | | | ] |
| (X) | - | | |

N
I...

FLEX SERIES
VERTICAL INSTALL.

DOOR / WINDOW (JAMB)

FXV-15 | .)
REV. 9/13/16