Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Prestige Series\Prestige Ser
Author: goughbrian

r

_(V)	1/2"
4"

COVER TRIM

1 3/4"

1 3/4"
_4"	1/2"

DF016

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
BUTYL  FLASHING  TAPE
(MAS . 025BF)

1/8" THK  HORSESHOE  SHIM ( SHIM.125)   OR EQUIVALENT
SEE NOTE 1 Z-METAL (ZC224)
TRIM FASTENER OR RIVET AT  12"   O. C. MAXIMUM

DRIP  FLASHING (DF030)

_I	1/ 4'
_\	GAP

DRIP FLASHING
_---	(DF016)
ALTERNATE DETAIL

1 . SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT   APPLICATIONS.
(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS

1 1/2"

1 1/ 2 "
4"

1 1/ 2 "

1 3/4"
_ZC224	135°--"7
c/1/2"
OPEN HEM

DF030

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

COVER TRIM (V)

I...

PRESTIGE SERIES
HORIZONTAL INSTALL.
d

SOFFIT (FRONT)

PSH-09
..)

REV. 6/20/17