Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Prestige Series\Prestige Ser
Author: goughbrian

r

1 1/2"

135 ·
5/ 8"

TC2O9

1/ 4: 12 MIN. SLOPE

PARAPET FLASHING (V) BLOCKING (AS REQUIRED) TRIM CLEAT (TC2O9)
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

SPECIFIED UNDERLA YMENT (X)

SUBSTRATE

n,,;;,,,;.._
I. _..
_I.   .
I.
I _..•    •
_I . .

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

PARAPET

PSV-13

I...

REV. 11/15/18

..)