Prestige Series®
(Vertical Install.) Installation Guide

Prestige Series®
(Vertical Install.) Installation Guide

- Table of Contents -

Section	Page

General Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	i
Panel Details	1
Clip . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	2
Closures	3
Base	4
Sill	5
End Wall . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	6
Outside Corner . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	7
Inside Corner	8
Soffit (Front) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	9
Soffit (Back)	10
Soffit End Splice	11
End Splice (w/Trim)	12
Parapet	13
Door/Window (Head)	14
Door/Window (Jamb)	15
Door/Window (Sill)	16
Wall Penetration (3D)	17
Wall Penetration	18
Rigid Insulation	19

©2018 ASC Profiles.  All rights reserved.	Nov18

General Notes
The attached installation details are intended to be a design aid and do not depict all situations. Modifications are the responsibility of the designer/user and should take into account climate conditions such as wind and snow, governing code requirements, and the actual usage and maintenance of the structure.

Applications:
Prestige Series is designed to be used as a soffit panel, or as a wall panel installed in the vertical or horizontal orientation. It shall not be utilized for roof applications. Prestige Series can be used over solid substrates or over spaced supports. This installation guide depicts panels installed over solid substrate. Details for panels installed over spaced supports would be similar.

Flashings:
Where possible, flashings should be lapped away from prevailing winds. Certain flashings should be supported if it is likely that equipment (ladder, etc.) will be used against them. Check with AEP Span any time you intend to specify a prefinished flashing in a gauge or finish different than with Prestige Series. It is good practice to specify that all flashings be of the same material (gauge, color, finish) as the roof panels to ensure long-term durability. Field-painted flashings rarely equal the durability and colorfastness of factory baked-on paint systems. The enclosed details have minimized the use of exposed fasteners where possible. The edges of flashings have also been shown hemmed to strengthen and to minimize the exposure of cut edges.

Flashing design and fabrication is generally the responsibility of the contractor. For convenience, we have provided some typical flashing drawings on our website at http://www.aepspan.com/roof/prodDetailad08.ht ml?id=35 . Applicable Prestige Series flashing part numbers are referenced within this installation guide. Note that flashing shapes and dimensions may vary greatly based on project requirements. Installation details and flashings referenced within are for general design guidance only.

Condensation, Insulation, & Ventilation:
It is the designer's responsibility to determine the need and composition of condensation control materials including insulation and vapor retarders, as well as ventilation requirements.
Metal wall products are susceptible to condensation and its control should be carefully considered.

Thermal Movement:
Both panels and flashings must allow for thermal movement (expansion and contraction) of the materials, especially where long lengths are used. Appropriate gaps or other provisions must be provided to accommodate thermal movement.

Oil Canning:
Flat metal surfaces often display waviness commonly referred to as 'oil canning'. This can be caused by variations in raw material, processing variations, product handling, or variations in the installation substrate. Oil canning is a characteristic, not a defect, of panels manufactured from light-gauge metal. To reduce potential for oil canning, substrates should not deviate from a flat plane more than 1/4 inch in 20 feet, or 1/8 inch in 5 feet. Oil canning is not a cause for panel rejection. Additional technical information is available upon request.

References:
The Sheet Metal and Air Conditioning Contractors' National Association Inc. (SMACNA) manual is an excellent reference for sheet metal contractors. It’s guidelines for underlayments, gutter and downspout size requirements, and expansion/contraction of metals and flashing joints should be followed.

Technical Assistance:
Contact your AEP Span Sales Representative for additional information.

i

r	

NO REVEAL

1" REVEAL

2"  REVEAL

6"  REVEAL	i
J
WAVE (

-t-

i
I
<	I
I
I	12.0'  COVERAGE	1	
 	   I	J 	1.0· 1.5'
1   RIB (	4,	(	C	 	I
2   RIB		·  '  7	<
2 0

I-	10.0·	-j (

1.0' REVEAL

2 RIB t----

t 2.0 '   REVEAL

2 RIB t----

6,0'  REVEAL	7  	
J	J
C

-	3 , 0'	3.0·  7
2  RIB	J		

I...	PRESTIGE SERIES
VERTICAL INSTALL.
J	d 		
PANEL DETAILS	
		imleH	PSV-01	

.)	

r	

0 1/ 4'	TYP,
L
1'	o o]
t	.....
12'	2J
=	:::::;;;

J l	 	
C. . .    .    .    .    .    .    .     .	.		.		.		.		.		.		.		.		.		.		.		.    .
. .  . .  . .  . .  . .  . .  . .  . .  . .  . .  . .  . .  . . . . . .  . .  . .  . .  . .  . . . . ..

NOTES:
CLIP REQUIRED FOR MOST WIND LOAD CONDITIONS.
REFER TO PANEL ATTACHMENT SCHEDULES FOR PROPER CLIP/FASTENER SPACING & ASSOCIATED WIND LOAD CAPACITIES.
REFER TO AEP SPAN TECHNICAL BULLETIN #35 FOR ADDITIONAL INFORMATION REGARDING CLIP USAGE.	

_j

. .....	
....
. .			

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
CLIP	
		indeH		PSV-02	

.)	

r					
		6 X 1"			
		TEAR-OFF			
	
3 X 2"	PLUGS			
	TEAR-OFF PLUGS	

11 UP	

FULL		
		
10 UP			
	(J	
6 UP	11 UP		
	TOP SIDE CLOSURES		
10 UP		
			
6 UP		
					
			OPTIONAL: 1"W x 1/8"THK		
	TOP SIDE CLOSURE INSTALLATION		FOAM TAPE (MAS.125PE) TO SECURE CLOSURE PLUGS AGAINST PANEL & SEALANT.		

					

BOTTOM SIDE CLOS				
	INSTALLATION				
			
AD		
					
		CLOSU			

	NOTES:				
	- ALL CLOSURES SECURED AND				
	SEALED WITH POLYURETHANE SEALANT				

N
I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
CLOSURES	
		inde11	PSV-03	

.)	

REV. 6/15/17

r

4"

1"	1 7 /8"

135

1/2"

DFO24

·4.··.	I I
.   . .	I
I I I I I I I I

•   I
-    1

.    ·    1

. -     1
..	I

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)

BUTYL FLASHING TAPE (MAS.O25BF)
PANEL FASTENER

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT) DRIP FLASHING (DFO24)

..      I
.   -I
4
1·     .-    . 1

I . .

1 ·.

I

I .". I

.4	41	4	2
<I	4

.I	_- :
I . .
1 ."."
t

<I	4 ·

. <I
4

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

ind

BASE

PSV-04

I.	)

r				

_JJ,
..    I
..	I
. ..     ·1
.    .   I
..     I
.    .·.   1
••        I	SUBSTRATE
:..   1I
SPECIFIED UNDERLA YMENT (X)

....   1r1r	BUTYL  FLASHING   TAPE
(MAS.O25BF)
I
..  IJ..	PANEL FASTENER
.. I

I	INSIDE CLOSURE (SEALED &
..	SECURED WITH SEALANT)
•   • 1
••      I
SILL FLASHING (V)

..	I
..    I	ALTERNATE WALL MATERIALS
.    .·.   1
.   . I
..	I
. ..   ·1	 	f
 	    	 1/ 4 ' GAP
t

ON PROJECT CONDITIONS		

	

(X)	

-	

NOT BY AEP SPAN			
	(V)	-	DIMENSIONS VARY BASED			

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
SILL	
		inde11	PSV-05	

.)	

r

1 3/4"

3"

1/2"
1 1/2"

1 1/2"

1 1/2"

1 1/2"

JT107

. .d

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
.d	<I  .
·4
. ,.

<II '
4	.d

. <I

.d     .

<I

_    .d

(X) - NOT BY AEP SPAN

I  

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

END WALL

PSV-06
.)

r

1/2"

4"
0C111

1/2"f

4"

1 1/2"

1 1/2"

ZC224

1 1/2"

r, 	    	

SUBSTRATE SPECIFIED UNDERLA YMENT (X)

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
J	d 	

OUTSIDE CORNER

inde11	PSV-07

I.	)

r

1 1/2"

1 1/2"

1/2"
4"

ZC224

1 1/2"

4"

r, 		1/2" l	IC093

·
I
.          ·
...       ·
.    .

.. .· .'1
..·.- 1
..
..	I

.·.• ··
.·.
.   .  I

•.·. • ·
.    ·,
.·..·.1
.   .  I

·
<·..	--	
	1,
1'

I

I

,1
I
1

1

'

,I	SKINNING BUTYL TAPE OR SEALANT
1'	

=	=

·

T (X)

·•
.

3)
.

·

.

•

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
J	d 	

indeH

INSIDE CORNER

PSV-08

)

r

(V)	1/2"
4"
4"
COVER TRIM

1  3/4"	1   3 / 4"
135"7
1  3/4"	c/1/ 2"
OPEN HEM
4"	1/2"
DF030
DF016

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
BUTYL  FLASHING  TAPE
(MAS .0 25BF)

INSIDE  CLOSURE  (SEALED  &
SECURED  WITH SEALANT)

DRIP  FLASHING  (DF030)	I I • • •

I .
L	. ·.   . ·.  . · 	·.  . ·.   . ·.  . ·.  . ·.  . ·.   . ·.  . ·.  . ·.  . ·.  . ·.  . ·.   .
I

1/4'
GAP

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT
DRIP FLASHING
---	(DF016)	TRIM FASTENER W/SEALING WASHER
ALTERNATE  DETAIL	OR RIVET AT 12" O.C. MAXIMUM

COVER TRIM (V)

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
SOFFIT (FRONT)	
		indi	PSV-09
.)	

r

1/2"
4"

4"

1/2"l	IC093

ij 	,,
.	Q . .
¾	.   .•     .   .·     .    .·     .    .·     .    .•    . .•    .  .•     .   .·     .    .      .·    .    .·    .	.·.·
 		7
..
1 ·
I  ...
I .   .
I    .
1·
i,,>,l;
I            .
I· .
INSIDE  CORNER  TRIM  (ICO93)	I    •  •
I ' ,
PANEL  FASTENER	·1···
I ' ,
I           ••
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM
I.
CONTINUOUS   BEAD  OF  NON­	.,f
SKINNING  BUTYL   TAPE OR  SEALANT	I
SPECIFIED UNDERLA YMENT (X)

SUBSTRATE	l I
I	.·. I
I I	-       .          I I
I	· · I
I         1 •     •      I

(X)	-	NOT BY AEP SPAN	

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
SOFFIT (BACK)	
		indeH	PSV-10
..)	

r

3"	3"

1  3/4"	1  3/4"
1/2"	1 1/2"	1/2"
3"	1 1/2"
MT109	JT107

SUBSTRATE

SPECIFIED UNDERLA YMENT (X) END SPLICE (MT109)

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

J  TRIM  (JT107) REVEAL FLASHING (V)

.	a • ..	   	   	 	
·

1--
REVEAL SIZE PER ALTERN ATE DETAlL	PROJECT DESIGN

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
SOFFIT END SPLICE	
		indeH	PSV-11
.)	

r

4"

1 3/4"

1 1/2"
1/2" l
HT098

SUBSTRATE
.·.I	I	SPECIFIED   UNDERLA YMENT  (X)
. .	I
.·.+, I	BUTYL FLASHING TAPE
I	I	(MAS.O25BF)
. . . .	I
..	I  I  I	PANEL FASTENER
-
· • ·  •    I	I
••	I	I
.·     .·      1	I	INSIDE CLOSURE (SEALED &
. .	I	SECURED WITH SEALANT)
I
I :	END SPLICE /SILL FLASHING (HTO98)
.·.·:
TRIM FASTENER W/SEALING WASHER
I	OR RIVET AT 12" O.C. MAXIMUM
•   •       I	.
•    •     I	_;
·.·.1
r•• yI
••       I
..        I
....   I
•    I
••	I
=	= ••>•II
••       I

.      ·      1

 	      ••      I
!!_.  I

..	I
••       I
I

(X)	-	NOT BY AEP SPAN	

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
END SPLICE (W/TRIM)	
		indi	PSV-12
.)	

r

1 1/2"

135 ·
5/ 8"

TC2O9

1/ 4: 12 MIN. SLOPE

PARAPET FLASHING (V) BLOCKING (AS REQUIRED) TRIM CLEAT (TC2O9)
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

SPECIFIED UNDERLA YMENT (X)

SUBSTRATE

n,,;;,,,;.._
I. ..
.
I.
I ..•    •
I . .

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

inde11

PARAPET

PSV-13

I...

..)

r

4"

1/2"

1  3/4"
1/2"

135·	4"

135·

HT091

·-·-  1	1
••           I	I
••     I	I
I
·         ·       1	I
·.  ·.    1	I

I I
.         .   1
••	I

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)

.-.·1

••	I
••       I

••       I
••	I

·.·1
••	I

4

••       I

. .

I

••       I
_. _I.
I

1

17	I

1/    4 '	GAP

BUTYL FLASHING TAPE (MAS . O25 BF)

PANEL FASTENER

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT) HEADER TRIM (HT091)

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

DOOR / WINDOW (HEAD)

ind	PSV-14

I.	)

r

1/2"

135'

1 1/2"

1 1/2"

4"

1/2"

1 1/2" WC217

ZC224

1 1/ 2"	--------

SEALANT TRIM ANGLE
WALL CLOSURE

 ALTERNATE  DETAIL

SPECIFIED	]

OR RIVET AT 12" O. C. MAXIMUM WALL CLOSURE (WC217)

- NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

DOOR / WINDOW (JAMB)

indeH	PSV-15

I...

..)

r

1/2"
135·

4"

1/2"

1 1/2"

•   I
.                 ·1

.                 ·1
•  I
.  . .·1
•  I
.                  ·   1

.                 ·1
•   I

WALL CLOSURE (WC217)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

PANEL FASTENER SUBSTRATE
SPECIFIED UNDERLA YMENT (X)

.     ·1
•   I
.  . ·.1

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

DOOR / WINDOW (SILL)

inde11	PSV-16

I...

..)

r

DRIP FLASHING

TRIM  FASTENER W/SEALING
WASHER,  OR RIVET
SEALANT OVERLAP UPPER/LOWER
FLASHINGS

WALL  PENETRATION

SEAL PERIMETER ALL TRIM OVERL CONTINUOUS BE SKINNING BUTYL

I...

REV. 10/3/16

PRESTIGE SERIES
VERTICAL INSTALL.
J	d 	

WALL PENETRATION (3D)

imleH	PSV-17
.)

r			

..  I
.. I I
r1   ·. :
I       ..	I

I    .	I
1 · .
I
1·   ..	I
1 ·	I
I    .    .	I
-,

I I I I I I
        I
++-t'-
I	I
I
I    I 1 ·	I
.                   .    I
I	. I
I   1 >	I
I	I . .
1      ·  .	I
I I   .'.· I
I
.  . I
I	I			

SPECIFIED					
	UNDERLA YMENT (X)					
	SUBSTRATE					
	DRIP FLASHING (V)			------------ 7	-		
	CONTINUOUS BEAD OF NON-					
	SKINNING BUTYL TAPE OR SEALANT					
	UNDER COVER PERIMETER					
	SEAL PENETRATION PERIMETER					
	WITH POLYURETHANE SEALANT					
	WALL PENETRATION					
	OVERLAPPED PENETRATION COVER			 	   ,--		
				I		
	
PROVIDE SUFFICIENT CLEARANCE BETWEEN FLASHING & PENETRATION TO ACCOMODATE THERMAL MOVEMENT	,+		I I I I
I		
	TRIM  FASTENER W/SEALING
WASHER  OR RIVET			I I
I		

(X) - NOT BY AEP SPAN					
	(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS					

I...	PRESTIGE SERIES
VERTICAL INSTALL.
d 		
WALL PENETRATION	
		indeH	PSV-18	

.)	

r

H

SUBSTRATE RIGID  INSULATION (X)
SPECIFIED
UNDERLA YMENT (X) PANEL FASTENER ZEE  FLASHING  (V)

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS AND GAGE VARY BASED ON PROJECT CONDITIONS

PRESTIGE SERIES
VERTICAL INSTALL.
d 	

RIGID INSULATION

ind	PSV-19

I.	)

MANUFACTURING FACILITY:

Tacoma, Washington
2141 Milwaukee Way
Tacoma, WA 98421

Fontana, California
10905 Beech Avenue
Fontana, CA 92337

CORPORATE HEADQUARTERS:

ASC Profiles LLC 2110 Enterprise Boulevard West Sacramento, CA 95691

CUSTOMER SERVICE:
800-733-4955

Visit us at:
www.aepspan.com

©2018 ASC Profiles LLC.  All rights reserved.