Prestige Series®
(Horizontal Install.) Installation Guide

Prestige Series®
(Horizontal Install.) Installation Guide

- Table of Contents -

Section	Page

General Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	i
Panel Details	1
Clip . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	2
Closures	3
Base	4
Sill	5
End Wall . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	6
Outside Corner . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	7
Inside Corner	8
Soffit (Front) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	9
Soffit (Back)	10
End Splice	11
Parapet	12
Door/Window (Head)	13
Door/Window (Jamb)	14
Door/Window (Sill)	15
Wall Penetration (3D)	16
Wall Penetration	17
Rigid Insulation	18

©2018 ASC Profiles.  All rights reserved.	Nov18

General Notes
The attached installation details are intended to be a design aid and do not depict all situations. Modifications are the responsibility of the designer/user and should take into account climate conditions such as wind and snow, governing code requirements, and the actual usage and maintenance of the structure.

Applications:
Prestige Series is designed to be used as a soffit panel, or as a wall panel installed in the vertical or horizontal orientation. It shall not be utilized for roof applications. Prestige Series can be used over solid substrates or over spaced supports. This installation guide depicts panels installed over solid substrate. Details for panels installed over spaced supports would be similar.

Flashings:
Where possible, flashings should be lapped away from prevailing winds. Certain flashings should be supported if it is likely that equipment (ladder, etc.) will be used against them. Check with AEP Span any time you intend to specify a prefinished flashing in a gauge or finish different than with Prestige Series. It is good practice to specify that all flashings be of the same material (gauge, color, finish) as the roof panels to ensure long-term durability. Field-painted flashings rarely equal the durability and colorfastness of factory baked-on paint systems. The enclosed details have minimized the use of exposed fasteners where possible. The edges of flashings have also been shown hemmed to strengthen and to minimize the exposure of cut edges.

Flashing design and fabrication is generally the responsibility of the contractor. For convenience, we have provided some typical flashing drawings on our website at http://www.aepspan.com/roof/prodDetailad08.ht ml?id=35 . Applicable Prestige Series flashing part numbers are referenced within this installation guide. Note that flashing shapes and dimensions may vary greatly based on project requirements. Installation details and flashings referenced within are for general design guidance only.

Condensation, Insulation, & Ventilation:
It is the designer's responsibility to determine the need and composition of condensation control materials including insulation and vapor retarders, as well as ventilation requirements.
Metal wall products are susceptible to condensation and its control should be carefully considered.

Thermal Movement:
Both panels and flashings must allow for thermal movement (expansion and contraction) of the materials, especially where long lengths are used. Appropriate gaps or other provisions must be provided to accommodate thermal movement.

Oil Canning:
Flat metal surfaces often display waviness commonly referred to as 'oil canning'. This can be caused by variations in raw material, processing variations, product handling, or variations in the installation substrate. Oil canning is a characteristic, not a defect, of panels manufactured from light-gauge metal. To reduce potential for oil canning, substrates should not deviate from a flat plane more than 1/4 inch in 20 feet, or 1/8 inch in 5 feet. Oil canning is not a cause for panel rejection. Additional technical information is available upon request.

References:
The Sheet Metal and Air Conditioning Contractors' National Association Inc. (SMACNA) manual is an excellent reference for sheet metal contractors. It’s guidelines for underlayments, gutter and downspout size requirements, and expansion/contraction of metals and flashing joints should be followed.

Technical Assistance:
Contact your AEP Span Sales Representative for additional information.

i

r	

NO REVEAL

1" REVEAL

2" REVEAL

6"  REVEAL	i
J
WAVE (

-t-

i
I
<	I
I
I	12.0'	COVERAGE	1	
 	   I	J 	1.0· 1.5 '
1   RIB (	4,	(	C	 	I
2   RIB		·  '  7	<
2 0

I-	10.0·	-j (

1.0' REVEAL

2 RIB t----

t 2.0 '   REVEAL

2 RIB t----

6 ,0'     REVEAL	7  	
J	J
C

-	3 , 0'	3.0·  7
2  RIB	J		

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
J	d 		
PANEL DETAILS	
		indeH	PSH-01	

.)	

r	

0 1/ 4'	TYP,
L
1·
t
12·	2J
= :::::;;;

I	• I
i 	ii
DIRECTION	.       I	i \_,
EAVE	·.· 1 - -
I	I
.-    1 1	INSTALL
.
CLIP	..

PRESTIGE PANELS ARE INSTALLED FROM EAVE TO GROUND

NOTES:
CLIP REQUIRED FOR MOST WIND LOAD CONDITIONS.
REFER TO PANEL ATTACHMENT SCHEDULES FOR PROPER CLIP/FASTENER SPACING & ASSOCIATED WIND LOAD CAPACITIES.
REFER TO AEP SPAN TECHNICAL BULLETIN #35 FOR ADDITIONAL INFORMATION REGARDING CLIP USAGE.	

(	

INSTALL NEXT PANEL			

N
I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
CLIP	
		inde11		PSH-02	

.)	

r					
		6 X 1"			
		TEAR-OFF			
	
3 X 2"	PLUGS			
	TEAR-OFF PLUGS	

11 UP	

FULL		
		
10 UP			
	(J	
6 UP	11 UP		
	TOP SIDE CLOSURES		
10 UP		
			
6 UP		
					
			OPTIONAL: 1"W x 1/ 8" THK		
			FOAM TAPE (MAS.125PE) TO		
	TOP SIDE CLOSURE INSTALLATION		SECURE CLOSURE PLUGS AGAINST PANEL & SEALANT .		

					

BOTTOM SIDE CLOS				
	INSTALLATION				
			
AD		
					
		CLOSU			

	NOTES:				
	- ALL CLOSURES SECURED AND				
	SEALED WITH POLYURETHANE SEALANT				

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
CLOSURES	
		iod@H	PSH-03	

.)	

REV. 6/20/17

r	

1 1/2"
1 1/2"

1 1/2"

ZC224

.  -I
.   I
. .·. 1
••      I
. -    1
-	I
:-r
. -    1
••       I

.   I
-   1
.    .·  .1

•   I
•-I

-    1
..	I
. . ·. 1
•   I
. -1

<1
A	<1
.   '  <1	A  <I.	A -
A
. <1

A	_. <1

1. SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT APPLICATIONS.
(X) - NOT BY AEP SPAN	

A

_<1		

<1	

A

.. 4	

 	
t	

1"	

4"

1 7 /8"
1/2"
135

DF024

SUBSTRATE

SPECIFIED UNDERLA YMENT  (X) BUTYL FLASHING TAPE (MAS . 025BF)
1/8"   THK  HORSESHOE  SHIM ( SHIM.125) OR EQUIVALENT. SEE NOTE 1

Z-METAL (ZC224)

TRIM FASTENER OR RIVET AT 12 " O. C. MAXIMUM

SILL FLASHING (DF024)

p

PRESTIGE SERIES PANELS ARE INSTALLED FROM EAVE TO GROUND.		

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
BASE	
		indeH	PSH-04	

.)	

r					

1 1/2"	

1 1/2"			
		
1 1/2"			
		
ZC224			
					
			SUBSTRATE		
			SPECIFIED UNDERLA YMENT (X)		
			BUTYL FLASHING TAPE		
			(MAS.025BF)		
			1/8"	THK HORSESHOE SHIM		
			(SHIM.125) OR EQUIVALENT.		
			SEE NOTE 1		
			Z-METAL (ZC224)		
			TRIM FASTENER OR RIVET		
			AT 12" O.C. MAXIMUM		

. .. -1				
	 		 		1/  4'	GAP		
		t			
					
			SILL FLASHING (V)		
			ALTERNATE WALL MATERIALS		

1. SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH				
	MOUNT APPLICATIONS.				
	(X) - NOT BY AEP SPAN				
	(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS				

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
SILL	
		inde11	PSH-05	_	

)

r	

(X)	

-	

. 4

4	<1.
4

. :f!I
.·	· ·4
.

'. .	.   · .
_

. <1

4

.4

NOT BY AEP SPAN	

.
·	

. ·· t .
_	

3"

1 3/4"
1/2"

1 1/2"

JT107

PANEL FASTENER
SPECIFIED UNDERLA YMENT (X) SUBSTRATE

· · · · · · ·,· · · · · · · · · · · ·	· · ·
.       .	.	.	.	.	.	.       .	.	.       .	.	.	.	.       .	.       .	.	 .	.
·  _    ·       ·/	.    · _   ·	·  _    ·     .	·  _    ·       · _ ·    .	·  _    ·	·  _    ·    .	·  _    ·     .

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

J  TRIM   (JT1O7) SEALANT/ BACKER ROD			

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
END WALL	
		indeH	PSH-06	

.)	

r	

(X) -	

4"
.·I
.     _I
1/2"	••	I

4"	••      I
••       I
OC111	·. -I
••      I
I

r;	ill	".

SUBSTRATE SPECIFIED UNDERLA YMENT (X)

I
.  ..   . j;._.   .  ..   .  ..   .  ..   .  ..   .  ..  . .. .  ..   .  ..   .  .." ..' .  .  .  .  . " 	1i·ll   · .- ,,<_:<J
. . . . . . . . . . . . . . . . . . . . . . . . . . . . . .
---	l:_	---

PANEL FASTENER

CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

OUTSIDE  CORNER  TRIM (OC111)

NOT BY AEP SPAN			

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
OUTSIDE CORNER	
		indeH	PSH-07	

.)	

r

1/2"

4"

4"

r; 	

=	=

SUBSTRATE

SPECIFIED UNDERLA YMENT (X) INSIDE CORNER TRIM (ICO93)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

(X) - NOT BY AEP SPAN

PRESTIGE SERIES
HORIZONTAL INSTALL.
d 	

INSIDE CORNER

inde11	PSH-08

)

r	

(V)	1/2"
4"

COVER TRIM

1 3/4"

1 3/4"
4"	1/2"

DF016

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
BUTYL  FLASHING  TAPE
(MAS . 025BF)

1/8" THK  HORSESHOE  SHIM ( SHIM.125)   OR EQUIVALENT
SEE NOTE 1 Z-METAL (ZC224)
TRIM FASTENER OR RIVET AT  12"   O. C. MAXIMUM

DRIP  FLASHING (DF030)

I	1/ 4'
\	GAP

DRIP FLASHING
---	(DF016)
ALTERNATE DETAIL

1 . SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT   APPLICATIONS.
(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

1 1/2"	

1 1/ 2 "
4"

1 1/ 2 "

1 3/4"
ZC224	135°--"7
c/1/2"
OPEN HEM

DF030

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

COVER TRIM (V)		

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
SOFFIT (FRONT)	
		inde11	PSH-09	

..)	

r							

1 1/2"

ij 	
7 ....
,. .
I   . •• .
I . .
I,...•   .•
 	I.   .

I,... .
I..
,.
I        •   •

,...
t,. .
I   . •• .
I . .
I, •   .•
I,. .
.
I            .

"T	

1 1/2"

1 1/2"

ZC224			
		
1/2"									
		4"									
	
4"										
	1/2" l										
		
. .  ..  .  ..  .  .. .!·.		

.		
·.  .  .					

INSIDE CORNER TRIM (ICO93)										
	Z-METAL (ZC224)										
	TRIM FASTENER W/SEALING WASHER										
	OR RIVET AT 12" O.C. MAXIMUM										
	CONTINUOUS BEAD OF NON­										
	SKINNING BUTYL TAPE OR SEALANT										
	SPECIFIED UNDERLA YMENT (X)										
	SUBSTRATE										

(X) - NOT BY AEP SPAN										

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
SOFFIT (BACK)	
		inde11	PSH-10	

.)	

r						

3"	
3"		
			1  3/4"	
1 3/4"		
			1/2"	1 1/2"	1/2"		
			3"	1 1/2"		
			MT109	JT107		
				
SUBSTRATE		
				SPECIFIED UNDERLA YMENT (X)		
				END SPLICE (MT109)		

CONTINUOUS BEAD OF NON­		
				SKINNING BUTYL TAPE OR SEALANT		
				TRIM FASTENER W/SEALING WASHER		
				OR RIVET AT 12" O. C. MAXIMUM		
				
J TRIM (JT107)		
				REVEAL FLASHING (V)		
				.	a • ..	  	  	 			
			·			
			1--			
				REVEAL SIZE PER		
			ALTERN ATE DETAlL	PROJECT DESIGN		
	
(X)	
-	
NOT BY AEP SPAN			
	(V)	-	DIMENSIONS	VARY BASED ON PROJECT CONDITIONS				

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
END SPLICE	
		indeH	PSH-11	

.)	

r								

1 1/2"
1 1/2"			

1 1/2"				
				135"				
	1 1/2"			5/8"				
				TC209				

1/ 4: 12 MIN. SLOPE				

PARAPET FLASHING (V)							
	BLOCKING (AS REQUIRED)							
	
TRIM CLEAT (TC209)							
								
	TRIM FASTENER W/SEALING WASHER							
	OR RIVET AT 12" 0 .C. MAXIMUM							
	CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT							
	Z-METAL (ZC224)							
	SPECIFIED UNDERLA YMENT (X)							
	SUBSTRATE							

		..	I	I
I	. .
• •			

(X) - NOT BY AEP SPAN							
	(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS							

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
PARAPET	
		inde11		PSH-12	

.)	

r	

1 1/2"
1 1/ 2"

1 1/2"

ZC224

•   I
•      I
. . .·1
•     I I

I
•   I
·.·.1
•  I  I
<·,.. I
.   . 1

•   I
. . .·1

1. SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT APPLICATIONS.
(X) - NOT BY AEP SPAN					

4"		
				
1 3/4"		
		1/2"	
135·	1/2"
4"	135		
				HTO91		

PANEL FASTENER		
				SUBSTRATE		
				SPECIFIED UNDERLA YMENT (X)		
				BUTYL FLASHING TAPE (MAS .O25 BF)		
				1/8" THK HORSESHOE SHIM		
				( SHIM.125) OR EQUIVALENT.		
				SEE NOTE 1		
				Z-METAL (ZC224)		
				TRIM FASTENER OR RIVET		
				AT 12" O. C. MAXIMUM		
				HEADER TRIM (HT091)		
			
t			

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		DOOR / WINDOW (HEAD)	
		indeH	PSH-13	

..)	

r			

1/ 2"
135·
/,,
, ,
4"	I
I
1/2"	(	ill	\
'\  \4.  ...	.	. 	I
I
1 1/2"	I
--------	I
\	I
""','--- +	,	/
WC217
-----/',,
ALTERNATE DETAIL

r, 	

SUBSTRATE SPECIFIED
UNDERLA YMENT (X)

.	.	.      ._ .	._  .     .   ._ .	._ .    '.   .    .'.   . . _. .   .".   . . _. .  . ._. .  	
· 1. ·	.  . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .

PANEL FASTENER

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

WALL  CLOSURE  (WC217)

NOT BY AEP SPAN			

SEALANT		
				TRIM ANGLE (V)		
				WALL CLOSURE (V)		

]		

	

(X)	

-				

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		DOOR / WINDOW (JAMB)	
		indi	PSH-14	

..)	

r

1 1/2"

1 1/2"

1/2"

135"

1 1/2"	4"

ZC224	1/ 2"

1 1/2"

•   I
.                  ·    1

.                  ·   1

.  ..  ·1
•   I
.               ·1

·1
•  I

WALL CLOSURE (WC217)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

ETAL (ZC224) SUBSTRATE
SPECIFIED UNDERLA YMENT (X)

·1
•  I
.  . ·. 1

(X)	-	NOT BY AEP SPAN

PRESTIGE SERIES
HORIZONTAL INSTALL.
d 	

DOOR / WINDOW (SILL)

inde11	PSH-15

I...

..)

r

DRIP FLASHING

TRIM  FASTENER W/SEALING
WASHER,  OR RIVET
SEALANT OVERLAP UPPER/LOWER
FLASHINGS

WALL  PENETRATION

SEAL PERIMETER ALL TRIM OVERL CONTINUOUS BE SKINNING BUTYL

NOTE: VERTICAL INSTALLATION SHOWN ; HORIZONTAL INSTALLATION SIMILAR

PRESTIGE SERIES
HORIZONTAL INSTALL.
d 	

WALL PENETRATION (3D)

imleH	PSH-16

I.	)

r

SPECIFIED UNDERLA YMENT (X)

SUBSTRATE TRIM  FASTENER W/SEALING

WASHER  OR RIVET

CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT UNDER COVER PERIMETER

OVERLAPPED PENETRATION COVER

WALL  PENETRATION

PROVIDE SUFFICIENT CLEARANCE BETWEEN FLASHING & PENETRATION  TO ACCOMODATE  THERMAL MOVEMENT .

SEAL PENETRATION PERIMETER WITH  POLYURETHANE SEALANT

(X) - NOT BY AEP SPAN	

I...	PRESTIGE SERIES
HORIZONTAL INSTALL.
d 		
WALL PENETRATION	
		inde11	PSH-17
..)	

r

-

..
..
I I
1-

SUBSTRATE RIGID INSULATION (X)

H

SPECIFIED
UNDERLA YMENT (X)

I

I
tr
PANEL FASTENER ZEE  FLASHING  (V)
SUBGIRT

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS AND GAGE VARY BASED ON PROJECT CONDITIONS

PRESTIGE SERIES
HORIZONTAL INSTALL.
d 	

RIGID INSULATION

indeH	PSH-18

I.	)

MANUFACTURING FACILITY:

Tacoma, Washington
2141 Milwaukee Way
Tacoma, WA 98421

Fontana, California
10905 Beech Avenue
Fontana, CA 92337

CORPORATE HEADQUARTERS:

ASC Profiles LLC 2110 Enterprise Boulevard West Sacramento, CA 95691

CUSTOMER SERVICE:
800-733-4955

Visit us at:
www.aepspan.com

©2018 ASC Profiles LLC.  All rights reserved.