STEP	STEP
1	2

AT IBS.

\.,.....		SE HEMMING TOOL TO FIELD BEND TAB UNDER PANEL

STEP
3

APPLY 3/8" BEAD OF NON-SKINNING BUTYL SEALANT ON OUTSIDE MALE RIB AS SHOWN
4"	NARROW
/BATTEN CAP

MALE RIB OF
SELECT SEAM PANEL

'--		SELECT SEAM PANEL

FINISHED EAVE HEM

(#JC095)

CLEARANCE FOR THERMAL MOVEMENT PER CALCULATIONS	

N	SELECT SEAM
NARROW BATTEN
_j\	 	liL	
EAVE HEM	
		SSNB-05
.)	
REV. 4/17/20