Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Select Seam\SSNB\2020 SSNB A
Author: GOUGHBRIAN

ROOF JACK

GENERIC PANEL SHOWN	_ATION

ESS STEEL
WHEN USING	_CLAMP
^SUBSTRATE, ^WOOD	Y AEP-SPAN)
MUST BE 1" DIAM LARGER THAN R

3" MIN
BOTH  SIDES	_ECIFIED
DERLAYMENT
EE GENERAL NOTES)
ROOF JACK (DEKTITE REFER TO MANUFAC INSTRUCTIONS FOR IN

_NOTES:	LARGER THAN PIPE.
PENETRATIONS  SHOULD  BE CENTERED	^LOCATE ^ALL ^PIPE  ^IN IN   PANELS  IF  AT  ALL  POSSIBLE	^THE ^BROAD ^FLAT ^OF
SUBSTRATE   MUST  BE CUT  OUT	^THE ^PANEL ^.
ENOUGH SO THAT ROOF JACK IS ONLY ATTACHED TO ROOF PANEL .

ROOF CURB	_ASTENERS
ING TO FIX SUBSTRATE.

UPHILL FLASHING DETAIL #SSNB-18

ROOF

GENER PANEL SH

ER PANEL MUST
D 9" MIN  UNDER B FLASHING.

FLASHING
L #SSNB-17

/

N

SELECT SEAM
NARROW BATTEN
^_j\	 	liL

ROOF PENETRATIONS

SSNB-16
.)

REV. 4 /17 /20