r

CONTINUOUS ZEE CLOSURE (#ZC22O) NOTCHED FOR RIB ONLY
NON-SKINNING BUTYL SEALANT  AT ENDS
-    FILL  ALL GAPS

CONTINUOUS DOUBLE BEAD BUTYL TAPE

CONTRUCTION SEALANT (NOT BY AEP-SPAN)

.QlM '.8'.
#RG145: 4:

DIM 'B'
113: 6"
115: 7"
117: 8"

ENGINEERED  FASTENER	TRIM
(NOT BY AEP-SPAN)
ETS
o.c.

URE

NON-SKINNING BUTYL SE AT ENDS  OF  ZEE  & PANEL PENETRATIONS.
SPECIFIED	 	-
UNDERLAYMENT --
(NOT  BY  AEP-SPAN)	SUBSTRATE

EQUALLY SPACED'	6"x7/ 8" CONTINUOUS
BLE BEAD BUTYL TAPE
PANCAKE FASTENERS
(3)   FOR  13  1/4"
&   17   1/4"	- ZEE CLOSURE MUST BE CONTINUOUS
(4)  FOR 22   1/2"	AND BE NOTCHED FOR PANEL RIBS.
WIDE PANELS    )	- BATTEN MUST STOP AT OUTSIDE FACE
OF ZEE CLOSURE AND NOT PASS THROUGH.	

N
A Bluescope Steel Company
I...	SELECT SEAM
WIDE BATTEN

HEAD WALL	
		SSWB-09
.)	

REV. 5/4/12