Title: C:\Users\goughbrian\Desktop\Installation Details 2008\Select Seam\SELECT SEAM - ALL DETAILS 3-30-12 Model (1)
Author: goughbrian

r

EQUALLY SPACED ANCAKE FASTENERS (3) FOR 13 1/4"
& 17 1/4"
(4) FOR 22 1/2"
WIDE PANELS

SPECIFI UND
(NOT  BY  A

CLIP

JOGGLE CLEAT	C09 BETWEEN RI
SEALANT AT

3/8" BEAD BUTYL SEAL

---

-
g"	MIN. LAP

I...

  	 	r	 	
N
A Bluescope Steel Company
REV. 5/4/12

SELECT SEAM
WIDE BATTEN

PANEL LAP

SSWB-13
.)