Title: C:\Users\goughbrian\Documents\PRODUCT FOLDERS-----------------\INSTALLATION DETAILS - Master Files\Flex Series\Flex Series - Ho
Author: goughbrian

r | | | | . I .  ·^I, . | |
| | | 1/2" | | |
| | | 4" | | |
| | | 1/2" | | |
| | | 4" | | |
| | | OC111 | | |
| | | CLIP FASTENER | | |
| | | PANEL CLIP | | |
| | | SUBSTRATE | | |
| | | SPECIFIED UNDERLA YMENT (X) | | |
| | | OPTIONAL FIELD FORMED | | |
| | | CLOSURE COVER TRIM (X) | | |
| | | OUTSIDE CLOSURE (SEALED & | | |
| | | SECURED WITH SEALANT) | | |
| | | CONTINUOUS BEAD OF NON­ | | |
| | | SKINNING BUTYL TAPE OR SEALANT | | |
| | | TRIM FASTENER W/SEALING WASHER | | |
| | | OR RIVET AT 12" O. C. MAXIMUM | | |
| | | OUTSIDE CORNER TRIM (OC111) | | |
| (X) | - | NOT BY AEP SPAN | | |

N
I...

FLEX SERIES
HORIZONTAL INSTALL.

OUTSIDE CORNER

| FXH-08 | .)
REV. 6/19/17